HW2

COE 546

Map

Description automatically generated

Solution:

ISP 5%


show ip route

A screenshot of a computer program

AI-generated content may be incorrect.


R8 10%

show ip route eigrp




R5 20%

show ip route eigrp




show ip eigrp topology




ASBR1 20%

show ip route




ASBR2/ABR1 10%

show ip route




R2 10%

Show ip route ospf




show ip ospf neighbor




R10 5%

show ip route ospf




R4 10%

show ip route rip



**For the following, please show the configuration of the first 4 ports only:**

Show ports configuration and Primary/Secondary RB for SW 7 2.5%



Vlan 10

A screenshot of a computer program

AI-generated content may be incorrect.

Vlan 20

A white text with black numbers and numbers


AI-generated content may be incorrect.

Show ports configuration and Primary/Secondary RB for SW10 2.5%


A screen shot of a computer

AI-generated content may be incorrect.

Vlan 10



Vlan 20



Show ports configuration for SW 8 2.5%

A screenshot of a computer program

AI-generated content may be incorrect.

Show ports configuration for SW 9 2.5%

A screenshot of a computer program

AI-generated content may be incorrect.